

**7MTT – Oracle 7mode to CDOT Work Instructions**

**Authors:** David Ng

**Contributors:**

**Document Version:** V2

**Date:** April 2015

**Status:** Published

**CONFIDENTIAL INFORMATION**

This document contains information proprietary to Thomson Reuters and may not be reproduced, disclosed or used in whole or part without express permission of Thomson Reuters.

© Thomson Reuters 2013

Contents

[1 Introduction 3](#_Toc430699777)

[1.1 Management Summary 3](#_Toc430699778)

[1.2 Change History 3](#_Toc430699779)

[1.3 Distribution List 3](#_Toc430699780)

[1.4 Glossary 3](#_Toc430699781)

[2 7Mode to CDOT Migration 5](#_Toc430699782)

[2.1 High Level Migration Steps 5](#_Toc430699783)

[2.2 Pre-requisites 5](#_Toc430699784)

[2.3 Vserver and LIF creation 5](#_Toc430699785)

[2.3.1 Create Vserver (replace hyphen with underscore in vserver rootvolume name) 5](#_Toc430699786)

[2.3.2 Create LIF with default route and failover group 6](#_Toc430699787)

[2.4 DNS configuration 6](#_Toc430699788)

[2.4.1 Setup DNS on a Vserver 6](#_Toc430699789)

[2.5 Create service account if required 6](#_Toc430699790)

[2.6 Enable Protocols 6](#_Toc430699791)

[2.6.1 Enable CIFS if required 6](#_Toc430699792)

[2.6.2 Enable NFS if required 6](#_Toc430699793)

[2.7 Start the Migration 7](#_Toc430699794)

[2.7.1 Login to 7MTT 7](#_Toc430699795)

[2.8 Post cut-over activities 26](#_Toc430699796)

[2.8.1 Create job schedule and snapshot policy for SNAP volume(s) 26](#_Toc430699797)

[2.8.2 Create export policies (nfs only) 26](#_Toc430699798)

[2.8.3 Create the default export-policy (nfs only: repeat this command for every nfs client) 26](#_Toc430699799)

[2.8.4 Create export policy rule (nfs only: repeat this command for each nfs volume and nfs client) 26](#_Toc430699800)

[2.8.5 Rename export policy & configure snapshot policy(CIFS only) 27](#_Toc430699801)

[2.8.6 Delete snapshot policies which were created by 7MTT (nfs only) 27](#_Toc430699802)

[2.8.7 Delete snapshot which where created by migration (NOSNAP volumes only) 27](#_Toc430699803)

[2.8.8 Rename junction paths (Only required when older versions of 7MTT are used) 27](#_Toc430699804)

[2.8.9 Setup snap autodelete on volumes (run for each SNAP volume) 27](#_Toc430699805)

[2.9 QoS Policy Group Creation 28](#_Toc430699806)

[2.9.1 Create QoS policy group and apply it at the volume level (create one QOS policy for each volume) 28](#_Toc430699807)

[3 Snapvault Configuration 29](#_Toc430699808)

[3.1 Cluster and Vserver Peering 29](#_Toc430699809)

[3.1.1 Confirm that cluster peering has been enabled 29](#_Toc430699810)

[3.1.2 Create the cluster peer (skip this step if cluster peering has been configured) 29](#_Toc430699811)

[3.1.3 Confirm if vserver peering has been configured 29](#_Toc430699812)

[3.1.4 Create vserver peering on the destination system (skip this step if vserver peering has been configured) 29](#_Toc430699813)

[3.1.5 Accept the vserver peering on the source system 29](#_Toc430699814)

[3.2 SnapVault configuration 29](#_Toc430699815)

[Volumes names in TR have ‘SNAP’ or ‘NOSNAP’ incorporated into them. SNAP volumes must have snapvault confirgured for disk based backups. NOSNAP volumes do NOT require backups. 29](#_Toc430699816)

[3.2.1 Create secondary volumes for SnapVault as type “DP” on the destination cluster 29](#_Toc430699817)

[3.2.2 Create a cron job schedule if it does not exist in the destination 30](#_Toc430699818)


[3.2.3 Configure a snapmirror policy on the destination 30](#_Toc430699819)

[3.2.1 Initialize SnapVault relationship on the destination 30](#_Toc430699820)

# Introduction

## Management Summary

This document details the process used to migrate an Oracle Database from 7mode to CDOTwith 7MTT.



## Change History

|  |  |  |  |
| --- | --- | --- | --- |
| **Ver** | **Date** | **Author** | **Key Changes** |
| 1 | April 2015 | David Ng | Initial Version |

## Distribution List

|  |  |
| --- | --- |
| **Name** | **Role** |
| Storage Support |  |
| Storage Delivery |  |

## Glossary

|  |  |
| --- | --- |
| **Term** | **Definition** |
| cDOT | clustered Data ONTAP |
| Vserver | A logical storage virtual server, also known as a Storage Virtual Machine (SVM), which contains LIFs, Volumes, and configuration information such as access control details. |
| LIF | Logical Interface – a cDOT logical network interface with an IP address, assigned to a single Vserver. |
| 7MTT | 7mode Transition Tool – A tool used to migrate from 7mode to CDOT |
| WFA | OnCommand Workflow Automater – An automation framework application from NetApp, used for storage provisioning. |

# 7Mode to CDOT Migration

## High Level Migration Steps

|  |  |
| --- | --- |
| Create SVM and volume | Storage |
| Initialize snapmirror replication | Storage |
| Stop application during maintenance window | Application |
| Unmount source volumes during maintenance window | Platform |
| Final snapmirror sync/break during maintenance window | Storage |
| Update server mount info, e.g., ‘/etc/fstab’ | Platform |
| Mount new volume during maintenance window | Platform |
| Start application | Application |
| Verify | Application/Platform |

## Pre-requisites

* Confirm the target aggregate has sufficient capacity
* Confirm the source volume is 64 bit
* Register the target vserver hostname in DNS
* Make note of service accounts on the source so they can be created in destination
* Confirm there is network connectivity between the source and target
* Add the CDOT vserver name (not IP) to the source systems /etc/snapmirror.allow file
* Make note of qtree quotas sizes so they can be applied in destination
* Make note of the source volume language
* Make note of the backup volume size

## ****Vserver and LIF creation****

### Create Vserver (replace hyphen with underscore in vserver rootvolume name)

vserver create -vserver <vsname> -rootvolume <vsname>\_root -aggregate <aggrname> -ns-switch file -nm-switch file -rootvolume-security-style unix -language <language>

vserver show

### Create LIF with default route and failover group

network interface create -vserver <vsname> -lif <vsname>-lif-<lif#> -role data -data-protocol <protocol> -home-node <node> -home-port <port> -address <ip> -netmask <netmask> -status-admin up -firewall-policy mgmt -failover-group <group>

network routing-groups route create -vserver <vsname> -routing-group d<network>/<mask> -destination 0.0.0.0/0 -gateway <gateway>

vserver show

network interface show

network interface show -failover

network routing-groups route show –vserver <vsname>

## ****DNS configuration****

### Setup DNS on a Vserver

vserver services dns create -vserver <vsname> -domains <domainname> -name-servers <comma\_separate\_name\_server\_list>

vserver services dns show

## Create service account if required

security login role create -role <ROLE\_NAME> -cmddirname "<COMMAND>" -access <ACCESS\_TYPE> -vserver <vserver> #Repeat this command for each required command

security login create -username <USER\_NAME> -application ontapi -authmethod <AUTHENTICATION\_METHOD> -role <ROLE\_NAME> -vserver <vserver>

## ****Enable Protocols****

### Enable CIFS if required

cifs create -cifs-server <vsname> -domain <ad\_domain> -ou CN=Computers -status-admin up -vserver <vsname>

cifs show

cifs options show

### Enable NFS if required


vserver nfs create -vserver <vsname> -access true -v3 enabled

vserver nfs show


## ****Start the Migration****

### Login to 7MTT


Connect the 7MTT (https://<7MTT\_Server>:8443/transition) tool via web browser




* CLICK ‘Migrate’




* CLICK on the ‘Storage System’ button in the left pane:




* ADD storage systems to 7MTT (execute this step for the source and target storage systems):
* ENTER the FQDN of the filer
* CLICK ADD




* CLICK the ‘HOME’ tab -> CLICK ‘Get Started’




* CONFIRM that the source and destination storage systems are listed
* CLICK ‘Next’




* ENTER a name for the project
* CLICK ‘Continue’




* SELECT the source vfiler and volume(s):
* CLICK ‘Create Project and Continue’




* ENTER an IP to be used for replication traffic on the source filer
* CLICK ‘Next’




* The next window will ask if you want to run pre-check.
  + CLICK ‘Run Prechecks’



* Review the Report. You can ignore the warnings listed below. Resolve errors if they appear.
  + CLICK ‘Close’
  + CLICK ‘Next’




* SELECT a target vserver
* CLICK ‘Next’




**IMPORTANT: Make sure you enter the correct information in this section! Newer versions of 7MTT allow you to set junction path = volume name, this is the DCO standard. But, you need to modify the junction-path after the cut-over manually in older versions of 7MTT.**

* ENTER the destination aggregate
* ENTER the destination volume name
* SELECT ‘Use Clustered OTAP volume name’ from ‘Target Volume Mount Policy’ if drop down menu is available
* CLICK ‘Next’




NOTE: We are not migrating IP addresses


* CLICK ‘Next’




* CLICK ‘Create Schedule’, a popup box will appear
* ENTER a replication schedule (run off hours)
* CLICK CREATE




* The newly created schedule will appear
  + CLICK ‘Next’




* RUN PreCheck and make sure there are no errors
  + CLICK ‘Run Precheck’; REVIEW the output
  + CLICK ‘Close’
  + CLICK ‘Next’




* REVIEW the output
* CLICK ‘Save and go to Dashboard’




* A data transfer workflow will be displayed in the top of the page. The circle above ‘Baseline Data Copy’ will have a white fill color before your first transfer. It will have an orange fill color while the first transfer is running. Then a green fill color after your first successful transfer.
* CLICK ‘Run Pre-Check’; REVIEW output
* CLICK ‘Start Baseline’
* A popup window will appear, CLICK ‘yes’




* Execute an update transfer before the cutover window so that you have minimal changes to transfer during the cutover window:
  + CLICK ‘Update Now’




* Ensure the steps below are completed during the downtime window:
* The application/database has been shut down
* Source volumes have been unmounted
  + Start the cutover process:
  + CLICK ‘Apply Configuration’
  + A popup box will appear, CLICK ‘Continue’




* REVIEW log for errors
* CLICK ‘Close’



* CLICK ‘Complete Transition’
* A popup box will appear, CLICK ‘yes’
* A popup box will appear stating that the source volume will be made offline, CLICK ‘Continue’



* REVIEW the log output for a successful transition
* CLICK ‘Close’



## ****Post cut-over activities****

### Create job schedule and snapshot policy for SNAP volume(s)

job schedule cron create -name <volume\_name> -minute <min> -hour <hour>

volume snapshot policy create -vserver <vsname> -policy <volume\_name> -enabled true -schedule1 <volume\_name> -count1 7 -snapmirror-label1 snapvault -prefix1 sv\_<volume\_name>

job schedule cron show -name <vol\_name>

volume snapshot policy show –vserver <vsname>

### Create export policies (nfs only)

vserver export-policy create –vserver <vsname> –policyname <volume\_name>

### Create the default export-policy (nfs only: repeat this command for every nfs client)

vserver export-policy rule create -vserver <vsname> -policyname default

-clientmatch <nfsclient> -rorule sys -rwrule sys -superuser sys

### Create export policy rule (nfs only: repeat this command for each nfs volume and nfs client)

vserver export-policy rule create -vserver <vsname> -policyname <volume\_name> -clientmatch <nfsclient> -rorule sys -rwrule sys -superuser sys

#Use this command for SNAP volumes

volume modify -volume <volume\_name> -policy <volume\_name> -snapshot-policy <volume\_name> -vserver <vserver>

#Use this command for NOSNAP volumes

volume modify -volume <volume\_name> -policy <volume\_name> -snapshot-policy none -vserver <vserver>

volume show -vserver <vsname>

vserver export-policy rule show

### Rename export policy & configure snapshot policy(CIFS only)

volume show -vserver <vserver> -fields policy

vserver export-policy rename -vserver <vserver> -policyname <old\_policy> -newpolicyname <volume\_name>

volume show -vserver <vserver> -fields policy

#Use this command for SNAP volumes

volume modify -volume <volume\_name> -snapshot-policy <volume\_name> -vserver <vserver>

#Use this command for NOSNAP volumes

volume modify -volume <volume\_name> -snapshot-policy none -vserver <vserver>

### Delete snapshot policies which were created by 7MTT (nfs only)

snapshot policy show -vserver <vserver>

snapshot policy delete -vserver <vserver> -policy <policy\_name>

### Delete snapshot which where created by migration (NOSNAP volumes only)

volume snapshot show -vserver <vserver> -volume <volume\_name>

volume snapshot delete -vserver <vserver> -volume <volume\_name> –snapshot <snapshot>

### Rename junction paths (Only required when older versions of 7MTT are used)

volume unmount -vserver <vserver> -volume <volume\_name>

volume mount -vserver <vserver> -volume <volume\_name> -junction-path /<volume\_name>

volume show -vserver <vserver> -junction

### Setup snap autodelete on volumes (run for each SNAP volume)

volume modify -vserver <vsname> -volume <volname> -space-mgmt-try-first snap\_delete

volume snapshot autodelete modify -vserver <vsname> -volume <vol\_name> -enabled true

volume snapshot autodelete modify -vserver <vsname> -volume <vol\_name> -trigger snap\_reserve

volume snapshot autodelete show -vserver <vsname>

volume show -vserver <vsname> -fields space-mgmt-try-first

volume snapshot autodelete show -vserver <vsname>

## ****QoS Policy Group Creation****

### Create QoS policy group and apply it at the volume level (create one QOS policy for each volume)

qos policy-group create -policy-group <volname> -vserver <vsname> -max-throughput 6000iops

volume modify -vserver <vsname> -volume <volume> -qos-policy-group <volname>

qos policy-group show

volume show –vserver <vsname> -fields qos-policy-group

# Snapvault Configuration

## Cluster and Vserver Peering

### Confirm that cluster peering has been enabled

cluster peer show

### Create the cluster peer (skip this step if cluster peering has been configured)

cluster peer create -peer-addrs <remote\_ICL\_IP1,remote\_ICL\_IP2> -username admin

cluster peer show

### Confirm if vserver peering has been configured

vserver peer show

### Create vserver peering on the destination system (skip this step if vserver peering has been configured)

vserver peer create -vserver <destination\_vserver> -peer-cluster <source\_cluster> -peer-vserver <source\_vserver> -applications snapmirror

vserver peer show

### Accept the vserver peering on the source system

vserver peer accept -vserver <source\_vserver> -peer-vserver <destination\_vserver>

vserver peer show

## SnapVault configuration

### Volumes names in TR have ‘SNAP’ or ‘NOSNAP’ incorporated into them. SNAP volumes must have snapvault confirgured for disk based backups. NOSNAP volumes do NOT require backups.

### Create secondary volumes for SnapVault as type “DP” on the destination cluster

volume create -vserver <vserver> -volume <volume\_name> -aggregate <aggr\_name> -size <size> -security-style unix -space-guarantee none -percent-snapshot-space 0 -language <vol\_language> -type DP

volume show

### Create a cron job schedule if it does not exist in the destination

job schedule cron create -name xdp\_<hour> -minute 00 -hour <hour>

job schedule show

### Configure a snapmirror policy on the destination

snapmirror policy create -vserver <vserver> -policy <volume>

snapmirror policy add-rule -vserver <vserver> -policy <volume> -snapmirror-label snapvault -keep <retention#>

snapmirror show -destination-path \* -fields Schedule

snapmirror policy show

### Initialize SnapVault relationship on the destination

snapmirror create -source-path <source\_vserver>:<source\_volume> -destination-path <destination\_vserver>:<destination\_volume> -type XDP -schedule <schedule\_name> -policy <policy\_name>

snapmirror initialize -destination-path <destination\_vserver>:<destination\_volume>

snapmirror show